{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Vars","DAT_template","Instructions"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Vars","index":0,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Unused","C:\\Referncs\\"]
["Input file","C:\\Users\\svyst\\OneDrive\\Рабочий стол\\0_3b2c26f0.qdc"]
["Target File","H:\\La512\\GNDevia.dat.dat1"]

{"sheet":"DAT_template","index":1,"n_rows":1,"n_cols":5,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["##","Depth","Slope","Azimuth","Comment"]

{"sheet":"Instructions","index":2,"n_rows":44,"n_cols":2,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["Quickdraw export"]
[]
[]
["Кнопка запускает диалоговое окно в котором можно выбрать какие данные (глубина или код качества) из какого слоя данных вы хотите экспортировать и в каком формате (CSV или ESRI ASCII Grid).\nПри экспорте в CSV будет создан текстовый файл (разделитель запятая) с полями ID - номер по порядку; X - долгота в десятичных градусах; Y - широта в десятичных градусах; Depth(m)- глубина в метрах; либо ValCode - код качества вместо глубины.\nПри экспорте в ESRI ASCII Grid будет создано 2 файла с расширениями .grd и .prj Полученный растр можно загрузить во многие ГИС (например QGIS) и конвертировать в более быстрочитаемый формат.\nПри работе, скрипт создает двумерный массив, размер которого пропорционален площади прямоугольника вмещающего все обрабатываемые данные, что может приводить к вылету с ошибкой \"Out of memory\".  Бороться с ошибкой можно используя 64-битную версию Excel (позволяет использовать до ~3Гб RAM под массивы) или запуская скрипт отдельно для более глубоких папок в структуре данных QuickDraw. 64-битный эксель позволяет экспортировать всю площадь ОВХ без проблем.\nЕсли объем данных большой скрипт может работать несколько часов при этом Эксель будет в состоянии \"Не отвечает\". "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":" (360 / (2 ^ 23))","v":4.291534423828125E-5}]
[{"$f":" (360 / (2 ^ 24))","v":2.1457672119140625E-5}]
[]
[null,{"$f":"42.5*2","v":85}]